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	Term
	Definition

	Activity Centre
	A commercial precinct or shopping area as summarised in Attachment 4. 

	Arterial Road
	Refers to freeways, highways and declared main roads, which are managed by the Victorian Government, through Head of Transport for Victoria (as the co-ordinating road authority).

	Co-ordinating road authority
	The organisation which has the responsibility to co-ordinate works. Generally, if the road is a freeway or arterial road, this will be Head of Transport for Victoria. Generally, if the road is a municipal road, this will be Council.

	Council
	Refers to the City of Bayside or Bayside City Council

	Demarcation agreement
	A formal agreement between Council and another organisation that defines areas of responsibility.

	Motor vehicle
	Refers to a vehicle that is propelled by an in-built motor and is intended to be used on a roadway. This does not include a motorised wheelchair or mobility scooter which is incapable of travelling at a speed greater than 10 km/h and is solely used for the conveyance of an injured or disabled person.

	Major Pathway
	A high-use pedestrian footpath, usually located in an activity centre or near other select facility.  

	Municipal road(s)
	Road for which the municipal council is the co-ordinating road authority.  The Road Management Act 2004 imposes specific duties on the municipal council with respect to the inspection, repair and maintenance of these roads and associated road-related infrastructure.

	Non-road infrastructure
	Refers to infrastructure in, on, under or over a road, which is not road infrastructure. This includes (but is not limited to) such items as gas pipes, water and sewerage pipes, cables, electricity poles and cables, tram wires, rail infrastructure, bus shelters, public telephones, mailboxes, roadside furniture and fences erected by utilities, or providers of public transport.

	Other roads
	Include roads in state forests and reserves, and roads on private property. Municipal councils are not responsible for the inspection, repair or maintenance of these roads.

	Pathway
	Refers to a footpath, bicycle path, shared path or other area that is constructed or developed by Council for members of the public (not motor vehicles) to use.
Pathways may be further categorised as:
· Footpaths – pathways designated solely for use by foot traffic (and limited mobility devices such as wheelchair users)
· Bicycle pathways – pathways designated solely for use by cyclists, scooters and the like but excluding foot traffic, and
· Shared pathways – pathways designated for use by riders of bicycles, the riders of electric scooters and pedestrians.

	Public Road
	As defined by the Road Management Act 2004 and includes a freeway, an arterial road, a municipal road declared under section 14(1) of the Act and a road in respect of which Council has made a decision that it is reasonably required for general public use and is included on the Register of Public Roads.

	Plan
	Refers to this Road Management Plan.

	Road
	Has the same meaning as in the Road Management Act 2004, being inclusive of any public highway, any ancillary area and any land declared to be a road under section 11 of that Act or forming part of a public highway or ancillary area.

	Road infrastructure
	Refers to infrastructure which forms part of a roadway, pathway or shoulder, which includes structures and materials.

	Road-related infrastructure
	Refers to infrastructure installed or constructed by the relevant road authority to either facilitate the operation or use of the roadway or pathway, or support or protect the roadway or pathway.

	Road Reserve
	Refers to the area of land that is within the boundaries of a road.

	Roadside
	Refers to any land that is within the boundaries of the road (other than shoulders) which is not a roadway or pathway. This includes land on which any vehicle crossing or pathway, which connects from a roadway or pathway on a road to other land, has been constructed.
Example: any nature strip, forest, bushland, grassland or landscaped area within the road reserve would be considered roadside.

	Roadway
	Refers to the area of a public road that is open to, or used by, the public, and has been developed by a road authority for the driving or riding of motor vehicles. This does not include a driveway providing access to a public road, or other road, from adjoining land.

	Shoulder
	Refers to the cleared area, whether constructed or not, that adjoins a roadway to provide clearance between the roadway and roadside. This does not refer to any area that is not in the road reserve.





[bookmark: _Toc152582058][bookmark: _Toc152584801][bookmark: _Toc167799310][bookmark: _Toc190960641]Introduction
The Bayside Road Management Plan 2025 (RMP) was reviewed in accordance with the Road Management Act 2004 and Road Management (General) Regulations 2016. It was adopted by Council on ###.
[bookmark: _Toc152582059][bookmark: _Toc152584802][bookmark: _Toc167799311][bookmark: _Toc190960642]What is the purpose of this Plan

Section 50 of the Road Management Act 2004 sets the following objectives for a municipal road management plan:

1. To establish a system for our road management functions, which is based on policy, operational objectives and available resources.
2. To set a performance standard for our road management functions.

Although it is termed a ‘plan’ in the legislation, it is functionally an operational protocol document – describing the systems and rules we use to make decisions and meet obligations within our available resources. The plan forms part of a larger Asset Management framework related to maintenance and operations.

For the avoidance of doubt, this Plan is a road management plan for the purposes of s.39 of the Road Management Act 2004.

[bookmark: _Toc152582060][bookmark: _Toc152584803][bookmark: _Toc167799312][bookmark: _Toc190960643]Legislation guiding this Plan

In addition to the Road Management Act 2004, the plan also considers the following Acts, regulations and codes of practice:

· Local Government Act 1989/2020 
· Ministerial Codes of Practice
· Road Management (General) Regulations 2016 
· Road Management (Works and Infrastructure) Regulations 2015 
· Road Safety Act 1986 
· Wrongs Act 1958

[bookmark: _Toc152582061][bookmark: _Toc152584804][bookmark: _Toc167799313][bookmark: _Toc190960644]What is covered in this Plan?

The Plan is divided into six sections:

1. Introduction.
2. Rights and Responsibilities – covers legislation and local laws relevant to road management.
3. Road Management Systems - how we classify roads, streets and pathways – known as our asset hierarchy – and the plans and processes we use to maintain roads and road-related infrastructure.
4. Register of Public Roads – what’s in it, how to access it and the process for making changes.
5. Technical References. 
6. Attachments:
(a) Attachment 1, Road Hierarchy – Urban Roads
(b) Attachment 3, Pathway Hierarchy
(c) Attachment 4, Inspection Requirements
(d) Attachment 5, Inspection Frequencies
(e) [bookmark: _Toc152582062][bookmark: _Toc152584805]Attachment 6, Defect Intervention Levels and Repair Timeframes

[bookmark: _Toc167799314][bookmark: _Toc190960645]Updating the Plan

This Plan must be updated within a set period following a Council election. Outside of this cycle, changes may be required from time to time.

The following process will be used to manage these changes:

· If material changes are made to standards and specifications, a report will be presented to Council, along with a brief explanation as to why such changes are necessary. The review process must follow the steps as set out in the Road Management (General) Regulations 2016 Part 3 – Road Management Plans.
· When changes do not alter these technical aspects of road management, changes will be approved by the Director Environment, Recreation and Infrastructure.

These changes will be made in accordance with the processes prescribed by the Road Management Act 2004. To assist with version control, these changes will be numbered as follows:

· Versions presented to Council will be renumbered by whole numbers – for example, from Version 1.00 to 2.00.
· Those approved by the Director will be renumbered by decimals – for example, from Version 1.00 to 1.01.

[bookmark: _Toc152582063][bookmark: _Toc152584806][bookmark: _Toc167799315][bookmark: _Toc190960646]Exceptional Circumstances

Council will make every effort to meet its commitments under this Plan.

However, there may be situations or circumstances that affect Council's business activities to the extent that it cannot deliver on the service levels of the RMP. These include but are not limited to: natural disasters, such as fires, floods, or storms, or a prolonged labour or resource shortage, due to a need to commit or redeploy Council staff and/or equipment elsewhere or due to the effects of pandemic and or government intervention.

[bookmark: _Toc152582064][bookmark: _Toc152584807][bookmark: _Toc167799316][bookmark: _Toc190960647]Suspension of the Plan

In the event that the Chief Executive Officer (CEO) of Council has considered the impact of such an event on the limited financial resources of Council and its other conflicting priorities, and determined that the Plan cannot be met, then pursuant to Section 83 of the Wrongs Act 1958, the CEO will write to Council’s Officer in charge of the Plan and inform them that some, or all, of the timeframes and responses in Council’s Plan are to be suspended.

[bookmark: _Toc152582065][bookmark: _Toc152584808][bookmark: _Toc167799317][bookmark: _Toc190960648]Reinstatement of the Plan

Once the scope of the event/s have been determined, and the resources committed to the event response have been identified, then there will be an ongoing consultation between Council’s CEO and Council’s Officer responsible for the Plan, to determine which parts of Council’s Plan are to be reactivated and when.

[bookmark: _Toc152582066][bookmark: _Toc152584809][bookmark: _Toc167799318][bookmark: _Toc190960649]Communication and documentation around Plan suspension

Council will provide information/statements to residents about the suspension or reduction of the services under its Plan, including:

· How the work that will be done has been prioritised; and
· The period for which it is likely to be affected.

This information will be provided by the Council on its website where its Plan is located and other channels as appropriate such as press releases or social media.

Where Council has suspended, in part or whole, it’s Plan, associated documents (e.g. communications, meeting minutes, schedules, etc.) will be recorded and stored.

[bookmark: _Toc152582067][bookmark: _Toc152584810][bookmark: _Toc167799319][bookmark: _Toc190960650]Inspections and repairs during suspension of Plan

The suspension of the Plan will not necessarily mean that all inspections and repairs halt. However, it may mean that only certain categories of inspections and repairs are undertaken. These will be based on a risk assessment and resources available to the Council, taking into account the resources needed to address the impact of the trigger event. For example, some reactive inspections may take place and repair (temporary or permanent) of roads/footpaths which pose a high risk may be undertaken, depending on the resources available to the council and the accessibility of each asset.

[bookmark: _Toc152582068][bookmark: _Toc152584811][bookmark: _Toc167799320][bookmark: _Toc190960651]Responsibility for the Plan

Overall responsibility for administering and implementing the Plan rests with the Manager City Assets and Presentation. 
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[bookmark: _Toc152582070][bookmark: _Toc152584813][bookmark: _Toc167799322][bookmark: _Toc190960653]Public Roads

Public roads are defined in the Road Management Act 2004 as including:

· a freeway
· an arterial road
· a road declared under section 204(1) of the Local Government Act 1989
· a municipal road declared under section 14(1) of the Road Management Act 2004
· a road in respect of which Council has made a decision that it is reasonably required for general public use and is included on the Register of Public Roads.

[bookmark: _Toc152584814][bookmark: _Toc167799323][bookmark: _Toc190960654]Key stakeholders

The key stakeholders impacted by this Plan include:

· the general community (for recreation, sport, leisure and business)
· residents and businesses adjoining the road network
· pedestrians
· vehicle users with motorised vehicles, such as trucks, buses, commercial vehicles, cars and motorcycles
· users of smaller, lightweight vehicles, such as pedal-powered bicycles, motorised buggies, wheelchairs, prams and so on
· tourists and visitors to the area
· emergency agencies (Victoria Police, Fire Rescue Victoria, Ambulance Victoria, State Emergency Services)
· the military (in times of conflict and emergency)
· traffic and transportation managers
· managers of the road network asset
· construction and maintenance personnel, who build and maintain asset components
· utility agencies using the road reserve for infrastructure (water, sewerage, gas, electricity, telecommunications)
· state and federal governments, who periodically provide funding for roads.

[bookmark: _Toc152584815][bookmark: _Toc167799324][bookmark: _Toc190960655]Coordinating & Responsible Road Authority

Section 35 of the Road Management Act 2004 provides that a road authority has power to do all things necessary or convenient to be done for or in connection with the performance of its functions under the Act.

Section 36 of the Road Management Act 2004 outlines which road authority is the coordinating road authority. According to subsection (c), the coordinating road authority:

If the road is a municipal road, the municipal council of the municipal district in which the road or part of the road is situated.

However, there are instances where several authorities are responsible for components of the road within the road reserve. Section 37 of the Road Management Act 2004 identifies who is the responsible road authority in particular circumstances.

[bookmark: _Toc152584816][bookmark: _Toc167799325][bookmark: _Toc190960656]General Functions of a Road Authority

The general functions of a road authority are described within Section 34 of the Road Management Act 2004.

[bookmark: _Toc152584817][bookmark: _Toc167799326][bookmark: _Toc190960657]Rights of the Road User

The rights of public road users, which are legally enforceable, are set out in Sections 8 to 10 of the Road Management Act 2004.

[bookmark: _Toc152584818][bookmark: _Toc167799327][bookmark: _Toc190960658]Obligations of Road Users

[bookmark: _Toc152584819][bookmark: _Toc167799328][bookmark: _Toc190960659]General Usage

The common law requires that a road user must take reasonable care for their own safety (see Ghantous v Hawkesbury City Council).

The Road Safety Act 1986 sets out obligations on road users, including section 17A which requires that a person who drives a motor vehicle on, or uses, a highway must drive in a safe manner have regard for all relevant factors, including without limiting their generality, the following:

(a) physical characteristics of the road
(b) prevailing weather conditions
(c) level of visibility
(d) the condition of any vehicle the person is driving or riding on the highway
(e) prevailing traffic conditions
(f) the relevant road laws and advisory signs
(g) the physical and mental condition of the driver or road user.

Section 17A of the Road Safety Act 1986 also requires that a road user must take reasonable care:

(a) to avoid any conduct that may endanger the safety or welfare of other road users
(b) to avoid any conduct that may damage road infrastructure and non-road infrastructure on the road reserve
(c) to avoid conduct that may harm the environment of the road reserve
[bookmark: _Toc152584820][bookmark: _Toc167799329][bookmark: _Toc190960660]Incident Claims
	
[bookmark: _Hlk169271649]If a person proposes to make a claim in relation to a public road or infrastructure for which Council is the responsible road authority, that person should contact Council and Council will initiative respective investigation and insurance reporting processes.

In accordance with Section 110 of the Road Management Act 2004, Council is not legally liable for property damages where the value of the damage is equal to or less than the threshold amount.

In cases where the claim relates to assets Council does not own or is not responsible for on the road reserve, the person who proposes to make a claim must refer the claim to the other authority or person responsible for those assets.

[bookmark: _Toc152584821][bookmark: _Toc167799330][bookmark: _Toc190960661]Permits for work within a road reserve

In cases where an individual or organisation proposes to carry out works within the road reserve that may impede public access, or interfere with road infrastructure, they must apply for a ‘works within road reserve’ permit. There are some exemptions, as noted in the Road Management (Works and Infrastructure) Regulations 2015.

Local laws also require property owners to apply for a vehicle crossing permit if they plan to build a driveway.

In both cases, a fee applies to cover the costs of the administration and inspection of the work.

[bookmark: _Toc152584822][bookmark: _Toc167799331][bookmark: _Toc190960662]Obligation of others

There are several assets within the road reserve that Council does not have an obligation to inspect and/or maintain. These include:

· Non-road infrastructure – This includes (but is not limited to) such items as gas pipes, water and sewerage pipes, cables, electricity poles and cables, tram wires, rail infrastructure, bus shelters, public telephones, mail boxes, roadside furniture and fences erected by utilities, or providers of public transport.
· Single property stormwater drains – for drains constructed within the reserve that carry water from a single property to an outlet in the kerb, or other drain.
· Utilities – including, but not limited to; telecommunication, power, water, sewer, gas, and rail authority assets.
· [bookmark: _Hlk167866514][bookmark: _Hlk167866497]Roadside – as per Section 107 of the Road Management Act, Council has no “statutory duty or a common law duty to perform road management functions in respect of a public highway which is not a public road or to maintain, inspect or repair the roadside”, described as “any land that is within the boundaries of the road (other than shoulders) which is not a roadway or pathway”.  This includes landscaped tree plots within the footpath/pathway where the surface of the tree plot is not constructed with the intention of providing a trafficable pedestrian surface.
· Vehicle driveways – the vehicle crossing (including Cross-over), located between the carriageway and the property boundary, must be maintained by the adjoining property owner. However, Council is responsible for the portion of the driveway where the constructed pathway is reasonably required by the public in accordance with the following diagram:

Table 2.1 – Responsibility of Council and owners around crossover

[image: The image shows a typically vehicle cross-over and roadside. Red lines mark the edges of the different parts of the crossover and which party is responsible for them.  

The property owner is responsible for cross-over. Council are responsible for the road, kerb, and footpath. Council is responsible for works on the roadside, subject to s107 of the Road Management Act. ]

Where Council becomes aware of a hazard created by the defective condition of assets / infrastructure owned by another party, Council may at its absolute discretion:

· If located within assets / infrastructure for which Council is responsible (e.g. footpaths, road surfaces, etc.), or otherwise presents an immediate and significant risk to members of the public, undertake temporary measures to reduce the risk to members of the public until such time as the respective owner can implement permanent repairs (subject to Council’s available resources).
· Report in writing (e.g. email or letter) the presence of the hazard to the responsible party and request that repairs be implemented within a reasonable timeframe.
· Where repairs are not completed by the responsible party within the respective timeframe, Council may complete necessary repairs and invoice the responsible party for the costs.

However, where another party has a duty in relation to the asset / infrastructure, and Council has a discretionary power to take remedial action in relation to that matter, only that other party with the duty is liable in a subsequent proceeding, in accordance with s.104 of the Road Management Act 2004.
[bookmark: _Toc190960663]Road Management Assets
Bayside City Council is responsible for a range of infrastructure assets which supports its road management functions includes the road, footpaths, kerb and channel, traffic management, bridges, and street signage. 
[bookmark: _Toc190960664]Municipal Roads
[bookmark: _Toc190960665]Road Hierarchy

A hierarchy of road classifications has been adopted by Bayside to help define the typical levels of service that can be expected to apply to each category of road. 

The road hierarchy can be considered as a balance between a roads ‘traffic’ and ‘access’ functions. For example, the Nepean Highway services significant traffic volumes but provides very little direct property access, whereas a small residential cul-de-sac is exclusively used for property access. 

The hierarchy classification is used to determine the levels of service required, prioritise works programs and determine defect intervention responses. The greater road network hierarchy is as follows.  

Table 3.1 – Road hierarchy

	Road Hierarchy
	Function
	Coordinating Road Authority

	Category 0: Freeway
	Connect major areas and allow for travel at the maximum speed limit.
	State

	Category 1: Highway
	Connect major areas and arterial roads and may allow for travel at a higher speed limit.
	State

	Category 2: Arterial
	Connect highways and arterial road network and allow for travel between 60-70km/hr. 
	State

	Category 3: Sub-arterial
	Act as major routes in and around the municipality. They carry heavy traffic volumes and link the arterial network with lower order roads. They will have 2 clear traffic lanes (excluding parking) and can cater for (but may restrain) heavy and service vehicles.
	Council

	Category 4: Collector
	Collector roads carry significant traffic volumes and link residential areas with arterial roads or link between other collector roads. They will have 2 clear traffic lanes (excluding parking) and can cater for (but may restrain) heavy and service vehicles.
	Council

	Category 5: Access Major
	These carry only local traffic and are focused upon providing property access. They may have 1-2 lanes clear traffic lanes and cater for limited use by heavy and service vehicles. Most Bayside roads are included in this category. 
	Council

	Category 6: Access Minor
	These perform a very minimal function as local access roads and allow for limited use at low speeds. Rear or side laneways and cul-de-sacs are included in this category. 
	Council


[bookmark: _Toc190960666]Road Inventory
The road length by hierarchy and surface type for local roads in Bayside is as follows:

Table 3.2 – Road length by hierarchy – date last updated:		 9/01/2025

	Road Hierarchy
	Length (km)
	% of Network

	Category 3: Sub-arterial
	32.7
	8.7

	Category 4: Collector Road
	43.7
	11.6

	Category 5: Access Major
	279.9
	74.4

	Category 6: Access Minor
	19.9
	5.3

	Total
	376.2
	100



Table 3.3 – Road Length by Surface Type – date last updated:	9/01/2025

	
Surface Type
	Length (km)
	% of Network

	Sealed
	369
	98.1

	Unsealed
	7.2
	1.9

	Total
	376.2
	100



[bookmark: _Toc190960667]Unsealed Roads 

Most roads in Bayside were sealed several decades previous through subdivision or upgraded by Council to carry higher traffic volumes. Roadworks carried out by Council today generally seek only to renew those sealed surfaces. There remains a small number of gravel local roads, located south of Bay Road which total 1km in length.

Council considers traffic volumes to have stabilised in these roads and is aware that the informal state of these roads is preferred by a majority of residents abutting these streets, and by the general community. Council presently has no plan to seal these roads.  

[bookmark: _Toc190960668]Unconstructed Laneways 

Laneways are a sub-category of the ‘Access Minor’ category of the road hierarchy and characterised by narrow width, low speed limits, low traffic volumes, and serve a primarily ‘access’ function. Not all laneways in Bayside are proactively maintained by Council, and some are maintained by the adjacent property owners. 

Council’s responsibility over laneways is based on a consideration of whether they are ‘reasonably required for general public use’. A determination of whether a road is required for public use is based upon the following:

· whether the laneway services more than three properties
· whether it forms a critical link between two local roads or other laneways
· whether it forms a critical link to a council managed facility, such as a reserve
· whether it has historically been used as a thoroughfare (i.e. public highway)
· whether it is on land owned by Council
· whether Council has historically managed or maintained the laneway.
There are approximately 19km of laneways in Bayside, 13km of which are maintained according to the RMP. The remaining 6km are natural surface such as grass, earth, or sand, and has in some places has been fortified with gravel.

Council presently has no plans to upgrade these roads and laneways however upgrade may be considered on a case-by-case basis where:
· traffic volumes are predicted to increase significantly as a result of new development (such as a new multi-storey apartment building)
· This assessment is made by Council’s Traffic Management team (as per Bayside Planning Scheme clause 52.06-11) and shall generally require a developer to upgrade the laneway and contribute the asset to Council.
· traffic volumes have increased to a point where maintenance of a gravel laneway is no longer cost effective

[bookmark: _Toc190960669]Municipal Footpaths

Footpaths/pathways are located adjacent to roads managed by both Council and the Department of Transport and Planning (DTP). Council is the responsible road authority for pathways adjacent to arterial roads however and maintains these on behalf of DTP (with the exception of the Nepean Highway bicycle path). Footpaths through Council facilities or open spaces are not considered as part of this Plan and have their own maintenance regimes.

Footpaths in Bayside are generally constructed of concrete and asphalt although higher standards of construction or different materials have sometimes been used in high profile areas. Council shall seek to widen footpaths when carrying out renewal works to meet minimum DDA compliance.

The hierarchy of footpaths maintained by Council which support road management functions are as follows:

	Category
	Use

	Major
	Major footpaths are located in high traffic areas adjoining Bayside’s shopping precincts, select public and private high-use facilities, and the Beach Road/Esplanade shared user path. A full list of ‘major’ footpaths is included in Attachment 4. 

	Minor
	Formalised footpaths located in the road reserve in all areas not described above.

	Track
	Informal and non-constructed pathways located in the road reserve, often appearing as foot-trodden earth or sand. 

Council does not maintain tracks under the RMP. 


[bookmark: _Toc152584823][bookmark: _Toc167799332]
[bookmark: _Toc190960670]Unconstructed footpaths

Over the past several decades, Council has formalised most footpaths in Bayside although some foot-trodden ‘tracks’ remain. Most footpath works carried out today concern the capital renewal and maintenance of existing asphalt and concrete pathways, and limited maintenance of gravel paths. 

New constructed pathways in the road reserve are subject to Council’s ‘Footpath Treatments within the Road Reserve’ policy. This policy generally does not support new constructed footpaths south of Bay Road. 

[bookmark: _Toc190960671]Kerb and Channel

Bayside’s kerb and channel assets are a critical component of the drainage network, capturing and directing stormwater runoff from the road surface and property outlets into drainage pits.

The default construction material is concrete; however existing bluestone kerbs may be retained and reconstructed in areas where it has been historically dominant in accordance with Council’s Road Reserve Bluestone Replacement Policy.

[bookmark: _Toc190960672]Roads without kerb and channel

There are a small number of sealed and unsealed roads, which do not have a formal kerb and channel. Based upon historical observations, these roads can drain via infiltration or runoff being directed into existing pits or swales. Council has no plans to construct new kerb and channel assets where no specific drainage need has been identified.

[bookmark: _Toc190960673]Traffic Management

Council is responsible for signage, traffic signals, and passive traffic control assets (roundabouts, raised pavements, splitter islands) on municipal roads and at some interfaces with roads and rail. 

The Department of Transport and Planning maintains traffic signals on Council’s behalf.

[bookmark: _Toc190960674]Bridges

Council is responsible for three road bridges and two pedestrian bridges, not taking into consideration structures in reserves. They are all located over the Elster Canal in Brighton.

[bookmark: _Toc190960675]Drainage Assets
Council is responsible for all drainage pits located in Local Roads and all downstream pipes which drain Council roads, Council land, and private land.  

Council is also responsible for maintaining Council-owned pipes under arterial roads and highways. The Department of Transport and Planning is responsible for the maintenance of pits and pipes which take runoff from arterial roads and are not otherwise owned by Council.  
[bookmark: _Toc190960676]Road Management Systems

[bookmark: _Toc152584824][bookmark: _Toc167799333][bookmark: _Toc190960677]Background and Process

Road asset management involves managing both physical assets and uses and operation that have the potential to impact their condition. It applies to all road assets, including:

· the road – pavement and surface, as well as associated pathways, kerb and channel
· structures – bridges, culverts and traffic management devices
· road infrastructure – traffic signals and on-road electrical assets.

The aim of our road management system is to deliver a safe and efficient road network and meet community needs to the best of our ability, within available resources.

To create a road asset management system that would best meet our needs when inspecting, maintaining and repairing public roads, we used the following nationally recognised asset management frameworks:

· International Infrastructure Management Manual (IIMM) 2015, IPWEA
· IPWEA National Asset Management Systems (NAMS+)
· Other references, as listed in Technical References.

[bookmark: _Toc152584825]The system is designed to set the direction for our asset management activities. It is also linked to the annual business planning cycle.

[bookmark: _Toc152584827][bookmark: _Toc167799336][bookmark: _Toc190960678]Maintenance Management System

[bookmark: _Toc152584828][bookmark: _Toc167799337][bookmark: _Toc190960679]Maintenance Management

Council has a responsibility to all road users and the community to maintain public roads to a reasonably safe and suitable standard, within our available funds and resources. By developing long-term maintenance programs for our assets, we are better able to plan how we do this.

The following maintenance requirements shape our annual program and budget:

Routine maintenance standards
Standards vary across the network depending on the asset type and relevant risk factors, such as traffic volumes and composition, operating speeds, the susceptibility of assets to deterioration and the cost effectiveness of repairs. Competing priorities for funding are also relevant.

Defect intervention levels have been established using the VicRoads Standard Specification Section 750 and adapting it to local conditions.

The standards will be reviewed periodically to make sure they are adequate (see section 1.4).

Repair and maintenance works
Works must be completed within a specified time, depending on the severity and location of the defect. Response times are determined using local knowledge and experience and past performance as a guide. 

Response times are monitored and will be periodically reviewed (see section 1.4).

Temporary mitigation measures 
These are temporary works designed to reduce the risk of an incident, until such time as repair or maintenance works can be completed. 

Response times and safety measures – for example warning signs, flashing lights, and safety barriers – are determined by reference to the risk to safety, road type and traffic volume.

Emergency works 
Works that result from emergency incidents and must be undertaken immediately, for the safety of road users and the public. 

[bookmark: _Toc152584829]Emergency works might include traffic incident management, responses to fires, floods, storms and spillages, and any assistance required under the Victorian State Emergency Response Plan and Bayside Municipal Emergency Management Plan.

[bookmark: _Toc167799338][bookmark: _Toc190960680]Asset Management Plans

Our asset management plans guide the development of long-term asset renewal programs, helping us to plan and finance asset renewal and replacement.

[bookmark: _Toc152584830][bookmark: _Toc167799339][bookmark: _Toc190960681]Maintenance Surveys and inspections

A three-tier regime is used to inspect our road network assets. It covers safety issues, incidents, defects and condition inspections.

1. Reactive inspections (Request for Service or RFS)
These inspections are conducted in response to requests from the community. The inspection is carried out by a suitably qualified maintenance contractor employee and assessed according to the Hazard intervention levels, contained within Attachment 3.

2. Proactive Inspections
Regular timetabled inspections that are scheduled depending on traffic flow, the types of defects likely to impact the asset and the perceived risks of these defects. Assets are proactively inspected on the timeframes provided in Attachment 1. 


3. Condition Inspections
These inspections identify structural integrity issues which, if untreated, are likely to adversely affect the network overall. These issues may impact short-term serviceability, as well as the ability of the asset to perform for the duration of its intended life span.

These inspections are carried out in accordance with the Council’s asset management plans. They are undertaken by suitably qualified external contractors on a four yearly schedule.

[bookmark: _Toc152584831][bookmark: _Toc167799340][bookmark: _Toc190960682]Maintenance responsiveness and performance targets

The following information is recorded when we receive a Request for Service (RFS) from the community:

· Date the request was received
· Details of the request, including the location and nature of the reported hazard/defect (including any specific measurements if provided), name of the person making the request, copies of any photographs provided, etc.
· The personnel / department to which the request has been assigned for action
· Date by which the request must be actioned (based on the target response times specified in Attachment 3)
· Date when the request was actioned and/or completed (this typically involves someone carrying out an RFS inspection, as described in section 4.4, followed by any necessary repair works conducted).

By recording this information, we can monitor compliance against target response times – that is, the time it takes from receiving a request to carrying out an inspection and ultimately completing necessary works.

Customer requests will be inspected and assessed in accordance with timeframes specified in Attachment 3. Following are some possible outcomes from a reactive inspection:

· If a defect identified exceeds a Description / Intervention level specified in Attachment 3, a work order would be created with a date for completion of works in line with respective specified repair timeframes.
· If repairs are significant – for example, rehabilitation works are required – temporary mitigation measures may be undertaken to reduce the risk posed by the hazard/defect until the proper works can be undertaken (and subject to available resources).
· If the defect is assessed as below the Description / Intervention Level specified in Attachment 3, it would be noted (including why), but no remedial action will be conducted.

In all cases, the action taken would be noted against the original request.

Target response times and intervention times are based on ‘normal’ conditions. The same level of service would not apply in cases where the Plan has been suspended, under Section 1.5.
[bookmark: _Toc152584832][bookmark: _Toc167799341][bookmark: _Toc190960683]Asset Levels of Service

Five elements are taken into account when determining appropriate levels of service for the road network. These are:

· Community expectations;
· Technical standards;
· Organisational capacity;
· Performance measures and targets;
· [bookmark: _Toc152584833][bookmark: _Toc167799342]Safety of road and pathways users.

[bookmark: _Toc190960684]Register of Public Roads

Council maintains a register of public roads – called the Bayside Register of Public Roads – with the details of all public roads and ancillary areas for which we are responsible.

The Register of Public Roads is available on Council’s website. A hard copy can be made available at the Bayside City Council Corporate Centre (76 Royal Avenue, Sandringham) upon request.
[bookmark: _Toc152584834][bookmark: _Toc167799343][bookmark: _Toc190960685]Maintenance Demarcation (Boundary) Agreements

Where there are boundary agreements between us and other road authorities or private organisations, the schedule of roads affected, and agreements are listed in the Register of Public Roads.

We have agreements with the following road authorities and other transport-related authorities:

· Department of Transport and Planning (shared responsibility for arterial roads)
· Public Transport Victoria (bus infrastructure)
· VicTrack/Metro Trains Melbourne (railway-road interfaces) 
· City of Port Phillip (shared responsibility for Head Street)
· Glen Eira City Council (shared responsibility for Thomas Street)
· Kingston City Council (shared responsibility for Charman Road)
[bookmark: _Toc152584835][bookmark: _Toc167799344][bookmark: _Toc190960686]Roads not listed on the Register

The following roads are not listed on our Register of Public Roads:

· Roads which are the full responsibility of the state government, or a private enterprise;
· Unused roads for which we have not accepted responsibility;
· Roads drawn out on a plan of subdivision, until such time that we accept responsibility for these roads;
· Roads which we have not determined are reasonably required for general public use
[bookmark: _Toc152584836][bookmark: _Toc167799345][bookmark: _Toc190960687]Technical References

i. AS ISO 31000:2018 – Risk Management – Guidelines
ii. Integrated Asset Management Guidelines for Road Networks (AP-R202) 2002, Austroads Inc.
iii. International Infrastructure Management Manual (IIMM) 2015, IPWEA
iv. VicRoads Risk Management Guidelines
v. VicRoads Standard Specification Section 750 – Routine Maintenance
[bookmark: _Toc152584837]

[bookmark: _Toc152584840][bookmark: _Toc167799351][bookmark: _Toc190960688]Attachment 1: Inspection Requirements

	Inspection Type
	Purpose
	Inspection and Reporting Requirements

	Reactive – Request for Service (RFS) – Standard Response
	Reactive inspections are designed to confirm the nature of defects/hazards reported by members of the public or Council employees and identify any that exceed the intervention levels specified in Attachment 3.
	Performed by a Council/Contractor representative with knowledge of Description / Intervention Levels (Attachment 6) and road maintenance techniques who may then call in a higher level of expertise if necessary.
All Reactive inspections are conducted on foot, with defects measured and photographed as specified in Council’s Road Asset Inspectors Manual.
The report is required to identify specific safety defect, time first reported, time inspected and by whom, subsequent action and time of completion.

Reactive requests will be either ‘Urgent’ or ‘Standard’ (Non-urgent).

	Proactive Inspection
	Inspection undertaken in accordance with a formal programmed inspection schedule to determine if the road asset complies with the levels of service as specified.
A record of each asset is to be completed detailing the name of the inspector, the inspection date, and a description of any defects found that exceed the intervention levels specified in Attachment 3.
In addition, details of the inspection will be electronically recorded against the particular asset inspected.
	Proactive Inspections of roads are conducted via a slow-moving vehicle, while Proactive Inspections of all other asset types are conducted on foot, with defects measured and photographed as specified in Council’s Road Asset Inspectors Manual.
[bookmark: _Hlk160717274]Performed by a dedicated Plan inspector.





[bookmark: _Toc152584841][bookmark: _Toc167799352][bookmark: _Toc190960689]Attachment 2: Inspection Frequencies
NOTES:

1. If a ‘the proactive inspection is due on a Weekend or Public Holiday, the actual due date will be at the end of the month.  


	Asset Group
	Hierarchy Category
	Proactive Inspection Frequency

	Roads

	Sub-arterial, Collector, Major Access, and Minor Access roads (excluding laneways)
	Every 12 months

	
	Minor Access Roads
(including laneways)
	Every 36 months

	Footpaths

	Major Footpaths
	Every 6 months

	
	Minor Footpaths
	Every 12 months

	Kerb and Channel
	All kerb and channel
	Every 12 months

	Regulatory, Warning and Hazard Signs
	All road signage
	Every 12 months

	Bridges
	All road and pedestrian bridges
	Every 12 months

	[bookmark: _Hlk167800297]Overhanging vegetation
	All roads and footpaths
	Every 24 months





2

[bookmark: _Toc152584842][bookmark: _Toc167799353][bookmark: _Toc190960690]Attachment 3: Defect Intervention Levels and Response Times
[bookmark: _Hlk167800332]NOTES:

1. All ‘days’ stated are working days, excluding weekends and public holidays. 
2. All ‘months’ are based on the number of working days within. 
3. ‘Standard’ requests will be inspected within the ‘Initial Review’ response time. Following this Initial Review, they will be scheduled for action within the ‘Standard’ response time. 
4. If a ‘Standard’ Response Time elapses on a Weekend or Public Holiday, the actual due date will be the next Working Day. 
5. If a ‘Urgent’ Response Time elapses on a Weekend or Public Holiday, the actual due date will be as specified.    
6. In cases where a defect is not due to be repaired in less than 4 weeks, temporary measures such as installing warning signage, erecting barriers, or painting the defect with a bright contrasting colour, may be implemented at the time of identification to reduce the risk as much as is reasonably practicable until permanent repairs can be completed in line with the specified ‘Standard’ timeframe.

[bookmark: _Toc151559413][bookmark: _Toc152584843][bookmark: _Toc167799354][bookmark: _Toc190960691]Roads

	Defect type
	Description / Intervention Level
	Response Times

	
	
	Urgent/ 
Initial Review
	Standard

	Pothole
	Potholes in sealed pavement >25 mm in depth and >300 mm in diameter
	7 days
	45 days

	Pothole in unsealed road
	Potholes in sealed pavement >50 mm in depth and >300 mm in diameter
	7 days
	45 days

	Edge break
	Edge breaks >25mm extending 150mm laterally over a 1000mm in length
	7 days
	30 days

	Depressions / Rutting
	Depression/ruts in the traffic lane of a sealed pavement >50 mm in depth and requiring repair to an area less than 2m2
	7 days
	30 days

	
	Depression/ruts in the traffic lane of a sealed pavement >50 mm in depth and requiring repair to an area greater than 2m2
	7 days
	24 months

	Damaged or missing pit lids
	Damaged Council drainage pit lids (such that they are potentially structurally unsound).
	1 day
	45 days

	Blocked Drain
	Causing water to pond on trafficable sections of the road.
	1 day
	60 days

	Damaged or missing pit lids
	Damaged Council drainage pit lids (such that they are potentially structurally unsound)
	1 day
	45 days

	Vegetation overhead clearance
	Vegetation lower than 4.0m above the trafficable road surface
	7 days
	45 days


[bookmark: _Toc151559416][bookmark: _Toc152584846][bookmark: _Toc167799357]





[bookmark: _Toc190960692]Footpaths
NOTES: 
1. Pram crossings / ramps providing transition between road and footpath levels are treated as part of the footpath for the purposes of the application of description / intervention
2. A list of Major Footpaths is provided in Attachment 4. 

	Defect type
	Description / Intervention Level
	Response Times

	
	
	Urgent/ 
Initial Review
	Standard

	Vertical Displacement (concrete and brick footpaths)
	Major Footpaths
Vertical Displacement >20 mm in height
	7 days
	60 days

	
	Minor Footpaths
Vertical Displacement >25 mm in height
	7 days
	60 days

	Pothole or missing pieces (asphalt footpaths)
	Major Footpaths
Pothole >20mm in depth
	7 days
	60 days

	
	Minor Footpaths
Pothole >25mm in depth
	7 days
	60 days

	Vertical Displacement (asphalt footpaths)
	Vertical Displacement >75 mm in height over 1.2m straight edge
	7 days
	60 days

	Excessively Cracking
	More than 50% of concrete footpath bay is cracked
	7 days
	60 days

	Wide Cracking
	Cracking in footpaths >40 mm wide
	7 days
	60 days

	Damaged or missing pit lids
	Damaged Council drainage pit lids (such that they are potentially structurally unsound)
	1 day
	45 days

	[bookmark: _Hlk167800581]Vegetation overhead clearance
	Vegetation lower than 2.5m above the trafficable footpath surface
	7 days
	45 days












[bookmark: _Toc151559417][bookmark: _Toc152584847][bookmark: _Toc167799359][bookmark: _Toc190960693]Kerb and Channel

	Defect type
	Description / Intervention Level
	Response Times

	
	
	Urgent/ 
Initial Review
	Standard

	Displacement 
	Municipal Roads only
Vertical displacement – uplift section >50 mm
	7 days
	45 days

	Water ponding
	Municipal Roads only
Stormwater ponding in the kerb and channel that is:
· more than 20mm in depth
· over an extent of at least 1m 
· lasting 3 days or more
	-
	90 days


[bookmark: _Toc151559415][bookmark: _Toc152584845][bookmark: _Toc167799356]
[bookmark: _Toc190960694]Traffic Control Devices

	Defect type
	Description / Intervention Level
	Response Times

	
	
	Urgent/ 
Initial Review
	Standard

	Missing / Damaged Intersection Warning Signs 
	Intersection Warning Signs are missing, illegible or damaged making them substantially ineffective. 
	2 hours
	-

	Missing / Damaged Signage (all other signs)
	Regulatory, warning and hazard signs missing, illegible or damaged making them substantially ineffective. 
	2 hours
	45 days

	Missing / Damaged Guard Rail or fencing
	Guard rail/fence damaged or missing making them substantially ineffective or obstructing the road or footpath 
	2 hours
	45 days

	Missing / Damaged Pavement Markings
	Pavement markings which are missing or faded making them substantially ineffective
	7 days
	45 days




[bookmark: _Toc190960695]Bridges and Culverts

	Defect type
	Description / Intervention Level
	Response Times

	
	
	Urgent/ 
Initial Review
	Standard

	Bridge & Culvert defects
	Visible damage likely to pose an immediate and significant risk to members of the public
	1 day
	45 days



[bookmark: _Toc190960696]Third Party Assets
	Defect type
	Description / Intervention Level
	Response Times

	
	
	Urgent/ 
Initial Review
	Standard

	Third Party Assets
	Defects resulting from third party works or service authority assets in the road or footpath which cause a hazard. 
	2 days
	60 days




[bookmark: _Toc190960697]Attachment 4: List of Major Footpaths
NOTES: 
1. The tables below describe areas or facilities where some footpaths are maintained as major footpaths. Not all footpaths within the areas described are major footpaths. 
2. ‘Major’ footpaths may include primary activity centre frontages, critical links, or other pathways Council has otherwise determined to be high use.  
Activity Centres
	Item
	Activity Centre Name
	Melway Reference

	1
	Martin Street / New St, Brighton
	M67 E5

	2
	Martin Street / Nepean Highway, Brighton
	M67 G7

	3
	Hawthorn Road / North Road, Brighton
	M67 K8

	4
	Landcox Street, Brighton East
	M67 J8

	5
	Thomas Street, Brighton East
	M68 B10

	6
	Hawthorn Road / Nepean Highway, Brighton East
	M67 K11

	7
	Nepean Highway / Centre Road, Brighton East
	M67 K12

	8
	Nepean Highway / South Road, Brighton 
	M77 D5

	9
	South Road, Brighton
	M77 C4 & D4

	10
	Bluff Road / South Road, Brighton East
	M77 B4

	11
	Hampton Street / South Road, Brighton East
	M76 G1

	12
	Hampton Street / Pine Street, Brighton
	M76 G1

	13
	Bay Street Shops, Brighton
	M67 F9 & F10

	14
	Bay Street / New Street, Brighton
	M67 D9

	15
	The Esplanade, Brighton
	M67 C10

	16
	Church Street Shops, Brighton
	M67 D11, E11, E12

	17
	Were Street Shops, Brighton
	M76 F3

	18
	Were Street Shops, Brighton
	M76 F2

	19
	South Road / Beach Road, Brighton
	M76 D3

	20
	Hampton Shopping Centre, Hampton
	M76 F6 – G4

	21
	Ludstone Street / Kingston Street, Hampton
	M76 J5

	22
	Widdop Cresent / Keith Street, Hampton East
	M77 C6 

	23
	Bluff Road / Highett Road, Hampton East
	M77 A8

	24
	Highett Road / Spring Road, Highett
	M77 C8

	25
	Highett Road / Middleton St, Highett
	M77 E9

	26
	Bay Road / Jack Road shops, Cheltenham
	M77 F11

	27
	Bay Road / Avoca Street Shops, Highett
	M77 C10

	28
	Bluff Road / Bay Road, Highett / Sandringham
	M77 A10

	29
	Sandringham Shops
	M76 G9

	30
	Beach Road / Georgiana Street, Sandringham
	M76 F8

	31
	Bluff Road, Spring Street, Sandringham
	M76 K12

	32
	Bluff Road, Edward Street, Sandringham
	M85 K1

	33
	Bluff Road / Love Street, Blackrock
	M85 K2

	34
	Black Rock Shops
	M85 K4

	35
	Balcombe Park Shops, Black Rock
	M86 C5

	36
	Beaumaris Concourse
	M86 D7

	37
	Keys St Shops, Beaumaris
	M86 E9

	38
	Seaview shops, Beaumaris
	M86 F5

	39
	Balcombe / Charman Road
	M86 H5

	40
	Weatherall / McNamara Street, Cheltenham
	M86 G3


Schools
	Item
	Asset Type
	Address
	Melway Reference

	1
	Beaumaris North Primary School
	188 Reserve Road, Beaumaris (also frontages to Mcdonald Street and Wood Street)
	M86 D4

	2
	Beaumaris Primary School
	99 Dalgetty Road, Beaumaris (also frontages to Herbert Street, Edith Street and Emily Street)
	M86 D7

	3
	Hampton East School
	2 Berend Street (also frontages to Dane Road and Seafoam Street) Hampton East.
	M77 C6

	4
	Black Rock Primary School
	2 Ferguson Street (also frontage to Arkaringa Crescent) Black Rock. 
	M86 A2

	5
	Brighton Beach Primary School
	19 Windermere Crescent (also frontage to Exon Street) Brighton
	M76 E1

	6
	Brighton Grammar School
	29 Grosvenor Street, Brighton (also frontages to Cadby Street and New Street)
266-570 New Street, Brighton
277 – 278 New Street, Brighton
80 Outer Crescent, Brighton
26 Young Street, Brighton
	M67 D10

	7
	Brighton Primary School
	59 Wilson Street (also frontage to Male Street) Brighton
	M67 F11

	8
	Brighton Secondary College
	80 A – 124 Marriage Road, Brighton East
213 – 239 Dendy Street, Brighton East
	M76 K1

	9
	Cheltenham Primary
	231 Charman Road, Cheltenham
	M86 H2

	10
	Elsternwick Primary School
	44 Murphy Street, Brighton
	M67 F5

	11
	Firbank Grammar School
	31 Outer Crescent (also frontages to Barkly Street Middle Crescent and Inner Crescent Brighton
45 – 51 Royal Avenue Sandringham
	M67 E9 


M76 J11

	12
	Gardenvale Primary School
	66 Landcox Street, Brighton East
	M67 K8

	13
	Haileybury College
	120 South Road (also frontage to Villeroy Street) Brighton East
	M76 G4

	14
	Hampton Primary School
	528 Hampton Street (also frontage to Ludstone Street) Hampton
	M76 G5

	15
	Sacred Heart Primary School
	11 Fernhill Road (also frontages to Sandringham Road and Bay Road) Sandringham
	M76 H9

	16
	Sandringham College 7-9 Campus
	356 Bluff Road (also frontage to Lawson Parade) Sandringham
	M77 A9

	17
	Beaumaris Secondary College
	455 Balcombe Road (Frontages to Lawson Parade and Landsell Avenue) Sandringham
	M86 C5

	18
	Sandringham College 10-12 Campus
	11 Holloway Road, Sandringham
	M77 A11

	19
	Sandringham East Primary
	9 Holloway Road, Sandringham
	M77 A11

	20
	Sandringham Primary School
	29 Bamfield Street (also frontage to Francis Street) Sandringham
	M76 H8

	21
	St Agnes Primary School
	18 Peterson Street (also frontage to Locinda Street, Clyde Street and Spring Road) Highett
	M77 C8

	22
	St Finbars Primary School
	88 Centre Road (also frontage to Wallen Street and Nepean Highway) Brighton East.
	M76 F4

	23
	St Joan of Arc Primary School
	30 Dendy Street (also frontages to Wallace Grove and New Street) Brighton. 
	M76 E1

	24
	St Leonards College
	163 South Road, Brighton East.
	M76 H3

	25
	St Marys Primary School
	59 Holyrood Street (also Bendigo Street and Hayward Grove frontages)
	M76 F4

	26
	Stella Maris Primary School
	47 South Road (also frontages to Hartley Street and new Street) Brighton
	M86 E6


Immunisation Centres
	Item
	Asset Type
	Address
	Melway Reference

	27
	Corporate Centre
	76 Royal Avenue, Sandringham 
	M76 K12

	28
	Beaumaris Community Centre
	88 Reserve Road, Beaumaris (also frontages to Victor Street and Cloris Avenue)
	M86 D7

	29
	AW Oliver Pavilion
	8-10 Little Avenue, Hampton East
	M77 B6

	30
	William Street Pavilion
	80 William Street, Brighton
	M67 G11



Preschool Centres
	Item
	Asset Type
	Address
	Melway Reference

	31
	St Michael's & All Angels Church Playground
	32 Dalgetty Road, Beaumaris 
	M86 E8

	32
	Goodstart Early Learning Beaumaris
	2 Emily Street, Beaumaris
	M86 D7

	33
	Beaumaris 3YO Kinder
	78 Dalgetty Road (also frontages to Gibbs Street and Haldane Street) Beaumaris
	M86 E7

	34
	Beaumaris Children’s Playhouse
	24 Grandview Avenue, Beaumaris
	M86 C5

	35
	Black Rock Preschool
	55 Bluff Road, Black Rock
	M85 K3

	36
	Brighton Baptist Kindergarten
	156 Bay Street (also frontage to Cochrane Street) Brighton
	M67 F9

	37
	Brighton Beach Early Learning Centre
	21 New Street, Brighton
	M76 E3

	38
	Brighton Early Learning Centre
	247 New Street, Brighton
	M67 D10

	39
	Brighton Kids
	309 Nepean Highway Brighton East
	M67 H8

	40
	Brighton Juniors Childcare
	75 Wilson Street, Brighton
	M67 F11

	41
	Brighton Playroom Assoc.
	58 Wilson Street (also frontage to Male Street) Brighton
	M67 F11

	42 
	Cross Street Playgroup
	665 Hampton Street (also frontage to Were Street) Brighton
	M76 G3

	43
	East Beaumaris Kindergarten
	60 Wells Road, Beaumaris 
	M86 G6

	44
	Gordon Street Preschool
	17-19 Gordon Street, Beaumaris
	M86 G4

	45
	Grange Road Preschool
	66 Grange Road, Sandringham
	M76 K9

	46
	Only About Children
	461-463 Bluff Road, Hampton
	M77 A5

	47
	Hampton Children’s Playhouse
	12 Willis Street, Hampton
	M76 F5

	48
	Hampton Community Kindergarten
	1A Myrtle Road, Hampton
	M76 J7

	49
	Helen Paul Kindergarten
	33 Kingston Street, Hampton
	M76 J5

	50
	Holy Trinity Kindergarten
	8 Thomas Street, Hampton
	M76 G6

	51
	Hunt Memorial Kindergarten
Hunt ELC
	103 Cochrane Street, Brighton
	M67 F6

	52
	Hurlingham Park Preschool
	1 Palmer Avenue, Brighton East
	M67 J11

	53
	Jack and Jill Kindergarten
	26 Grandview Avenue, Beaumaris
	M86 C5

	54
	Janet Mundy Kindergarten
	6 Fern Street, Black Rock
	M85 K1

	
56
	Kids Company
	206 Tramway Parade, Beaumaris
	M86 F5

	57
	Kids Company
	139 Bay Road, Sandringham
	M76 K10

	58
	Larmenier Bluff Kids Playgroup
	453 Bluff (also frontages to Fewster Road and Raynes Park) Road Hampton
	M77 A6

	59
	Livingston Street Kindergarten
	1 Livingston Street, Highett
	M77 E8

	60
	Nagel Preschool
	59-61 Sandringham Road (also frontage to Victory Street) Sandringham
	M76 K9 

	61
	North Brighton Kindergarten
	145A Cochrane Street (also frontage to Cross Street) Brighton
	M67 F5

	62
	Olive Phillips Kindergarten
	Bodley Street, Beaumaris
	M86 E8

	63
	Olympic Avenue Kindergarten
	28 Olympic Avenue, Cheltenham
	M77 F12

	64
	Beis Efraim College Limited
	453 New Street, Brighton
	M67 E6

	65
	Goodstart Early Learning
	43 Cochrane Street, Brighton
	M67 F8

	66
	Sandringham Childcare
	5 Sandringham Road, Sandringham
	M76 G9

	67
	Sandringham Children’s Playhouse
	3 Beaumont Street, Sandringham
	M76 G9

	68
	St Johns Kindergarten
	14-16 Darcy Avenue, Sandringham
	M77 B12

	69
	St Marys Preschool Centre
	187 Dendy Street (also frontage to Hughes Street), Brighton East
	M76 J1

	70
	St Peters Kindergarten
	1 Moffatt Street, Brighton (also frontage to Were Street)
	M76 E2

	71
	Wilsons St Kindergarten
	11 Wilson Street, Brighton
	M67 F10

	72
	Yeshivah Preschool
	132 Marriage Road, Brighton East
	M77 A1



Maternal and Child Health Centres
	Item
	Asset Type
	Address
	Melway Reference

	73
	Beaumaris
	28 Bodley Street, Beaumaris
	M86 E8

	74
	Brighton 
	1A Cochrane Street, Brighton
	M67 E9

	75
	Brighton East 
	1 Palmer Avenue, Brighton East
	M67 J11

	76
	Hampton 
	483 Hampton Street, Hampton
	M76 G5

	77
	Highett
	1 Livingston Street, Highett
	M77 D8

	78
	Sandringham
	6-8 Waltham Street, Sandringham
	M76 G9


Other
	Item
	Asset Type
	Address
	Melway Reference

	79
	Corporate Centre
	76 Royal Avenue, Sandringham
	M76 K12

	80
	Beaumaris Library
	96 Reserve Road, Beaumaris
	M86 D6

	81
	Brighton Library and Council Chambers
	Boxshall Street and Wilson Street frontages
	M67 F11

	82
	Hampton Library
	1D Service Street, Hampton
	M76 G6

	83
	Sandringham Library
	2-8 Waltham Street, Sandringham
	M76 F9

	84  
	Beach Road Shared User Path
	Beach Road and Esplanade, between the Middle Brighton Baths, Brighton and Charman Road, Beaumaris
	Between M67 C10 and M86 H7



image1.jpeg




image2.png
Roadside
*subject to 5107 RMA





image3.png
(03) 9599 4444

PO Box 27, Sandringham VIC 3191 Ba Side

bayside.vic.gov.au XTY COUNCIL
_~




